- Processing
- p5.js
- Processing.py
- Processing for Android
- Processing for Pi

- Processing Foundation

This reference is for Processing 3.0+. If you have a previous version, use the reference included with your software in the Help menu. If you see any errors or have suggestions, please let us know. If you prefer a more technical reference, visit the Processing Core Javadoc and Libraries Javadoc.

Class | PWM
Name | ### set()
Examples |
Description | Enables the PWM output When no period is specified, a default 1 kHz (1000 Hz) is used.
Syntax |
    .set(period, duty)
    .set(duty)
Parameters |
period | int: cycle period in Hz
duty | float: duty cycle, 0.0 (always off) to 1.0 (always on)
Returns | void

Updated on January 1, 2021 03:38:10am EST
This work is licensed under a Creative Commons Attribution-NonCommercial-ShareAlike 4.0 International License.